견 적 서
2022년 07월 14일		명성사이언스
한국재료연구원 윤지희/선임 연구원님		대표자 : 임명원
		사업자등록번호 : 131-33-75180
T 055-280-3481, 010-2354-7564		인천광역시 남동구 은청로4-19 C동 236호
jhyoon@kims.re.kr		Tel: 032-818-8338 Fax: 032-432-6676
		E-mail: mss56815@naver.com
아래와 같이 견적 합니다.		www.ms0608.co.kr

품명 및 규격	수 량	단 가	공급가액
Materials Testing Machine
구 성 :-	1	19,500,000	19,500,000
1 LS-1
(1) Materials Testing Loading Frame
(2) Digital Control Console
(3) NEXYGEN-Plus. Software Package
2 YLC-1000-A1 1KN (100 kgf) Loadcell	1	4,800,000	4,000,000
3 TG38 90 degree Peel Test	1	1,900,000	1,800,000
4 TG74 Vice Grip for 180 degree Peel Test	1	1,200.000	800.000
5 P.C System	1	1,100,000	1,100,000
* 설치 및 시운전 (국내기준)
* 무상보증기간 : 설치완료 후 1년
	공급가	28,500,000
	부가세	2,850,000
	합 계	31,350,000
제작사/제작국 : LLOYD INSTRUMENTS LTD. / 미국
유효기간 : 30일 납 기 : 발주후30일 이내 결제조건 : 주문시 50% 출고시50% 기업은행 : 434-074998-04-011 담 당 자 : 임수정실장 1 LS1 - Universal Testing Machine (1) Universal Testing Loading Frame -. Max. Capacity : 100kgf (1,000N) max -. Crosshead travel range : 500mm -. Test speed : 0.01 – 2,400 mm/min. up to 100kgf -. Column distance : Single Column -. Min. Load Resolution : 0.0001N (0.00001kgf) -. Load accuracy : Better than +/- 0.5% of reading -. Extension resolution : Better than +/- 0.15 micron -. Data acquisition rate : 8 kHz -. Dimensions : 460mm (w) x 557mm (d) x 1001mm (h) -. Weight : 52kg net -. Desk-top Type, Requires Table, not included. -. 230VAC, 60Hz (2) 32 bit Microprocessor Digital Control Console -. For machine control and data display. -. 32bit Microprocessor. -. Saves up to 10 test programs, and saves up to 600 test results. -. Real-time values are displayed, and test results - load (or stress) & extension (or strain) are displayed simultaneously on 4-line backlit LCD panel. -. All parameters and functions for testing are installed, such as, unit selection, auto/manual return and auto zero setting, auto/manual break detection, peak/follow hold, and etc. -. Tests for load, stress, extension and strain can be easily performed without PC. (3) NEXYGEN- Plus. Material Test And Data Analysis Software Package -. Fully Windows 7 and compatible. -. For machine control and data analysis. -. Program format similar to spreadsheets for familiarity of use. -. Seamless OLE2 integration with Word, Excel, Access, PowerPoint and Outlook. -. Data exporting made easy with familiar drag and drop or cut and paste method. -. Right mouse button presents shortcut menus. -. Help menus and mouse rollover help. -. Statistics (SPC) are available. -. All the international test methods for general material testing, -. 1,000 sample tests are available per batch. -. Test results can be converted to ASCII, LOTUS and other spread sheets. -. ‘TickIT’ Accreditation from ISO. -. Especially for custom-made program, such as, unlimited cycling test, load rate control test and strain rate control test.

합계금액(부가세별도) :  一金 이천팔백오십만원정 (￦28,500,000)